Sentinel Dual (High Power)
SDL 8000
INPUT		
Rated power	8000 VA	
Voltage	220-230-240 	
Frequency	50/60 Hz ± 5 Hz 	
Power factor	>0.98	
Current distorsion	≤5%	
BY PASS		
Voltage tolerance	180÷264 Vac (selectable in Economy Mode and SMART ACTIVE Mode) 	
Frequency tolerance	Selected frequency ± 5% (user configurable) 	
OUTPUT and INVERTER OUTPUT		
Rated power	8000 VA	
Active power	7200 W	
Number phases	1 	
Crest factor (Ipeak/Irms)	3 : 1 	
Waveform	Sinewave 	
Frequency	50/60 Hz selectable 	
Voltage distortion with non-linear load	<5% 	
Voltage distortion with linear load	<3% 	
OVERLOAD TIMES		
100% < Load < 110%	1 min 	
Load > 150%	0.5 s 	
BATTERIES		
Typical recharge time	2÷4 h 	
ENVIRONMENTAL		
Color	Dark grey 	
Safety compliance	EN 62040-1:2008; EN 62040-1/EC:2009; EN 62040-1/A1:2013 and Directive 2014/35/EU 	
EMC compliance	EN 62040-2 and Directive 2014/30/EU 	
Accessories provided	2 output supply cables 10 A; 1 plug IEC-16 A; software; serial cable; tools for mimic panel 	
Protection rating	IP20 	
Protections	Overload - short-circuit - overvoltage - undervoltage - temperature - low battery	
Line-Interactive/Smart Active efficiency	98% 	
Noise (at 1 m)	<45 dBA at 1 m 	
Operating temperature	0 ÷ 40 °C	
Relative humidity	<95% no condensing	
DATA		
Weight	94 kg	
Dimensions (h w d)	2x(455x175x660)/2x175(4U)x483x660 mm