Sentinel Power Green
SPM 6
INPUT		
Voltage	220-230-240 Vac 	
Frequency	50/60 Hz +/- 10 Hz 	
BY PASS		
Voltage tolerance	160 - 276 Vac (selectable in Economy Mode or Smart Active Mode) 	
Frequency tolerance	Selected frequency ±10% 	
OUTPUT and INVERTER OUTPUT		
Rated power	6000 VA	
Active power	5400 W	
Waveform	Sinusoidal 	
OVERLOAD TIMES		
100% < Load < 110%	5 min 	
100% < Load < 120%	1 min 	
125% = Load < 150%	10 sec 	
Load = 150%	0,1 sec 	
BATTERIES		
Type	VRLA AGM maintenance-free lead based 	
Typical recharge time	6-8 hours 	
ENVIRONMENTAL		
Color	Dark grey RAL 7016 	
Safety compliance	EN 62040-1:2008; EN 62040-1/EC:2009; EN 62040-1/A1:2013 and Directive 2014/35/EU 	
EMC compliance	EN 62040-2 and Directive 2014/30/EU 	
Protection rating	IP20 	
Protections	Overcurrent - short-circuit - overvoltage - undervoltage - temperature - excessive low battery	
Line-Interactive/Smart Active efficiency	98% 	
Noise (at 1 m)	4÷6 h40 dBA at 1 m 	
Operating temperature	0°C / +40°C	
DATA		
Weight	63 kg	
Dimensions (h w d)	708x262x654 mm