Multi Guard
GMT 120
INPUT		
Voltage	380-400-415 Vac, three-phase + N 	
Voltage tolerance	from 294 Vac to 520 Vac 	
Frequency tolerance	between 40 Hz and 70 Hz	
Power factor	>0.99	
Current distorsion	< 2%	
BY PASS		
Rated voltage	380-400-415 Vac, three-phase + N	
Voltage tolerance	from 323 Vac to 437 Vac 	
OUTPUT and INVERTER OUTPUT		
Rated power	15 kVA / 13.5 kW per  module VA	
Frequency	50 Hz / 60 Hz 	
ENVIRONMENTAL		
Safety compliance	EN 62040-1:2008; EN 62040-1/EC:2009; EN 62040-1/A1:2013 and Directive 2014/35/EU 	
EMC compliance	EN 62040-2 and Directive 2014/30/EU 	
Protection rating	IP20 	
Line-Interactive/Smart Active efficiency	up to 99% 	
Noise (at 1 m)	from ≤ 60 dBA to ≤ 62 dBA 	
Operating temperature	0 °C / +40 °C	
Relative humidity	20% - 90% non-condensing